**USB Commands**

**MIPI**

**Write Command**

Bw50,aa,dddd –> 0x50 = R2 Device/write, aa = register address, dddd = data word

**Read Command**

Br52,aa -> 0x50 = R2 Device/read, aa= register address

SPI

**Write Command**

Swxx,aa,dddd –> xx=any number (masked), aa = register address, dddd = data word

**Read Command**

Srxx,aa -> xx=anynumber (masked), aa= register address